# BOSL2
![BOSL2 Logo](images/BOSL2logo.png)

**The Belfry OpenScad Library, v2**

A library for OpenSCAD, filled with useful tools, shapes, masks, math and manipulators, designed to make OpenSCAD easier to use.

Requires OpenSCAD 2021.01 or later.

- **NOTE:** BOSL2 IS BETA CODE.  THE CODE IS STILL BEING REORGANIZED.
- **NOTE2:** CODE WRITTEN FOR BOSLv1 PROBABLY WON'T WORK WITH BOSL2!

[![Join the chat at https://gitter.im/revarbat/BOSL2](https://badges.gitter.im/revarbat/BOSL2.svg)](https://gitter.im/revarbat/BOSL2?utm_source=badge&utm_medium=badge&utm_campaign=pr-badge&utm_content=badge)


## Documentation

You can find the full BOSL2 library documentation at: https://github.com/BelfrySCAD/BOSL2/wiki


## Installation

1. Download the .zip or .tar.gz release file for this library.  Currently you should be able to find this at https://github.com/BelfrySCAD/BOSL2/archive/refs/heads/master.zip
2. Unpack it. Make sure that you unpack the whole file structure. Some zipfile unpackers call this option "Use folder names". It should create either a `BOSL-v2.0` or `BOSL2-master` directory with the library files within it.  You should see "examples", "scripts", "tests", and other subdirectories.
3. Rename the unpacked main directory to `BOSL2`.
4. Move the `BOSL2` directory into the apropriate OpenSCAD library directory for your platform:
    - Windows: `My Documents\OpenSCAD\libraries\`
    - Linux: `$HOME/.local/share/OpenSCAD/libraries/`
    - Mac OS X: `$HOME/Documents/OpenSCAD/libraries/`
5. Restart OpenSCAD.


## Examples
A lot of the features of this library are to allow shorter, easier-to-read, intent-based coding.  For example:

[`BOSL2/transforms.scad`](https://github.com/BelfrySCAD/BOSL2/wiki/transforms.scad) Examples | Raw OpenSCAD Equivalent
------------------------------- | -------------------------------
`up(5)`                         | `translate([0,0,5])`
`xrot(30,cp=[0,10,20])`         | `translate([0,10,20]) rotate([30,0,0]) translate([0,-10,-20])`
`xcopies(20,n=3)`               | `for (dx=[-20,0,20]) translate([dx,0,0])`
`zrot_copies(n=6,r=20)`         | `for (zr=[0:5]) rotate([0,0,zr*60]) translate([20,0,0])`
`skew(sxz=0.5,syz=0.333)`       | `multmatrix([[1,0,0.5,0],[0,1,0.333,0],[0,0,1,0],[0,0,0,1]])`

[`BOSL2/shapes.scad`](https://github.com/BelfrySCAD/BOSL2/wiki/shapes.scad) Examples | Raw OpenSCAD Equivalent
---------------------------------- | -------------------------------
`cube([10,20,30], anchor=BOTTOM);` | `translate([0,0,15]) cube([10,20,30], center=true);`
`cuboid([20,20,30], rounding=5);`  | `minkowski() {cube([10,10,20], center=true); sphere(r=5, $fn=32);}`
`prismoid([30,40],[20,30],h=10);`  | `hull() {translate([0,0,0.005]) cube([30,40,0.01], center=true); translate([0,0,9.995]) cube([20,30,0.01],center=true);}`
`xcyl(l=20,d=4);`                  | `rotate([0,90,0]) cylinder(h=20, d=4, center=true);`
`cyl(l=100, d=40, rounding=5);`    | `minkowski() {cylinder(h=90, d=30, center=true); sphere(r=5);}`
`tube(od=40,wall=5,h=30);`         | `difference() {cylinder(d=40,h=30,center=true); cylinder(d=30,h=31,center=true);}`
`torus(d_maj=100, d_min=30);`      | `rotate_extrude() translate([50,0,0]) circle(d=30);`


