Welcome to Yuki I, a low power consumption and low noise server.
それぞれの雪の結晶は異なります。
vm_page_bootstrap: 987323 free pages and 53061 wired pages
kext submap [0xffffff7f8072e000 - 0xffffff8000000000], kernel text [0xffffff8000200000 - 0xffffff800072e000]
zone leak detection enabled
standard timeslicing quantum is 10000 us
mig_table_max_displ = 72
TSC Deadline Timer supported and enabled
YukiACPICPU: ProcessorId=1 LocalApicId=0 Enabled
YukiACPICPU: ProcessorId=2 LocalApicId=2 Enabled
YukiACPICPU: ProcessorId=3 LocalApicId=1 Enabled
YukiACPICPU: ProcessorId=4 LocalApicId=3 Enabled
YukiACPICPU: ProcessorId=5 LocalApicId=255 Disabled
YukiACPICPU: ProcessorId=6 LocalApicId=255 Disabled
YukiACPICPU: ProcessorId=7 LocalApicId=255 Disabled
YukiACPICPU: ProcessorId=8 LocalApicId=255 Disabled
calling mpo_policy_init for TMSafetyNet
Security policy loaded: Safety net for Rollback (TMSafetyNet)
calling mpo_policy_init for Sandbox
Security policy loaded: Seatbelt sandbox policy (Sandbox)
calling mpo_policy_init for Quarantine
Security policy loaded: Quarantine policy (Quarantine)
Copyright (c) 1982, 1986, 1989, 1991, 1993, 2015
The Regents of the University of Adelaide. All rights reserved.

HN_ Framework successfully initialized
using 16384 buffer headers and 10240 cluster IO buffer headers
IOAPIC: Version 0x20 Vectors 64:87
ACPI: System State [S0 S3 S4 S5] (S3)
PFM64 0xf10000000, 0xf0000000
[ PCI configuration begin ]
YukiIntelCPUPowerManagement: Turbo Ratios 0046
YukiIntelCPUPowerManagement: (built 13:08:12 Jun 18 2011) initialization complete
console relocated to 0xf10000000
PCI configuration changed (bridge=16 device=4 cardbus=0)
[ PCI configuration end, bridges 12 devices 16 ]
mbinit: done [64 MB total pool size, (42/21) split]
Pthread support ABORTS when sync kernel primitives misused
com.Yuki.YukiFSCompressionTypeZlib kmod start
com.Yuki.YukiTrololoBootScreen kmod start
com.Yuki.YukiFSCompressionTypeZlib load succeeded
com.Yuki.YukiFSCompressionTypeDataless load succeeded

YukiAMDCPUPowerManagementClient: ready
BTCOEXIST off
wl0: Broadcom BCM4331 802.11 Wireless Controller
5.100.98.75

FireWire (OHCI) Lucent ID 5901 built-in now active, GUID c82a14fffee4a086; max speed s800.
rooting via boot-uuid from /chosen: F5670083-AC74-33D3-8361-AC1977EE4AA2
Waiting on &lt;dict ID=&quot;0&quot;&gt;&lt;key&gt;IOProviderClass&lt;/key&gt;&lt;string ID=&quot;1&quot;&gt;
IOResources&lt;/string&gt;&lt;key&gt;IOResourceMatch&lt;/key&gt;&lt;string ID=&quot;2&quot;&gt;boot-uuid-media&lt;/string&gt;&lt;/dict&gt;
Got boot device = IOService:/YukiACPIPlatformExpert/PCI0@0/YukiACPIPCI/SATA@1F,2/
YukiIntelPchSeriesAHCI/PRT0@0/IOAHCIDevice@0/YukiAHCIDiskDriver/SarahI@sTheBestDriverIOAHCIBlockStorageDevice/IOBlockStorageDriver/
Yuki SSD TS128C Media/IOGUIDPartitionScheme/Customer@2
BSD root: disk0s2, major 14, minor 2
Kernel is LP64
IOThunderboltSwitch::i2cWriteDWord - status = 0xe00002ed
IOThunderboltSwitch::i2cWriteDWord - status = 0x00000000
IOThunderboltSwitch::i2cWriteDWord - status = 0xe00002ed
IOThunderboltSwitch::i2cWriteDWord - status = 0xe00002ed
YukiUSBMultitouchDriver::checkStatus - received Status Packet, Payload 2: device was reinitialized
MottIsAScrub::checkstatus - true, Mott::Scrub
[IOBluetoothHCIController::setConfigState] calling registerService
AirPort_Brcm4331: Ethernet address e4:ce:8f:46:18:d2
IO80211Controller::dataLinkLayerAttachComplete():  adding YukiEFINVRAM notification
IO80211Interface::efiNVRAMPublished():
Created virtif 0xffffff800c32ee00 p2p0
BCM5701Enet: Ethernet address c8:2a:14:57:a4:7a
Previous Shutdown Cause: 3
NTFS driver 3.8 [Flags: R/W].
NTFS volume name BOOTCAMP, version 3.1.
DSMOS has arrived
en1: 802.11d country code set to &#039;US&#039;.
en1: Supported channels 1 2 3 4 5 6 7 8 9 10 11 36 40 44 48 52 56 60 64 100 104 108 112 116 120 124 128 132 136 140 149 153 157 161 165
m_thebest
MacAuthEvent en1   Auth result for: 00:60:64:1e:e9:e4  MAC AUTH succeeded
MacAuthEvent en1   Auth result for: 00:60:64:1e:e9:e4 Unsolicited  Auth
wlEvent: en1 en1 Link UP
AirPort: Link Up on en1
en1: BSSID changed to 00:60:64:1e:e9:e4
virtual bool IOHIDEventSystemUserClient::initWithTask(task*, void*, UInt32):
Client task not privileged to open IOHIDSystem for mapping memory (e00002c1)
System Integrity Check: 100% Success 
[OK] Linux Yuki-I 5.10.60-v7l+ #1449 SMP Wed Aug 25 15:00:44 BST 2021 armv7l GNU/Linux 
[OK] CPU Cores
[OK] Random Access Memory
[OK] USB Interfaces
[OK] Network Interfaces


Boot Complete.